
HOW TO PAIR YOUR FOB TO YOUR MCOMPASS TABLET

1. Click start 🡪 Control Panel 🡪 Hardware and Sound 🡪 Add a Device
2. Look for Medspira AMP-SPP and click next



1. Click “Enter a Device’s Pairing Code”
2. Enter pairing code “1234” click next
3. Should say “device successfully added”

CHECKING THE PORT OF THE FOB (Steps should be taken from here for troubleshooting as well)

1. Start 🡪 Control Panel 🡪 Hardware and Sound 🡪 View Devices and Printers
2. Click on Medspira AMP-SPP (as should have been added)
3. Click on Properties
4. Click on hardware tab
5. Under Device Functions it should read “Standard Serial Over Bluetooth Link (COM**X**)
6. **X** represents the portal that the FOB is on (should be a number 1-10)
7. Open the mcompass software
8. Click on administrator and log in (top right corner)
9. Click on the Blue Tooth tab
10. Switch COM to corresponding with **X** from above (same number 1-10)



1. Click Connection Test
2. Results should read “Bluetooth connection established”